**Publisher | Editors**

HEWI

Marketing + Sales

HEWI Heinrich Wilke GmbH

PO Box 1260

D-34442 Bad Arolsen

Phone: +49 5691 82-0

presse@hewi.de

www.hewi.com

**Reprint free of charge - copy requested**

**Range 270 bicolour -**

**Elegant contrasts on the door**

The HEWI hardware range 270 is the perfect result of design, technology and quality. Combined with the bicolour rose, this creates an exciting play on the door. Deep matt black in contrast to the metallic stainless steel accents make the combination of rose and lever handle so unique.

Deliberately set accents with bicolour

Consisting of two materials, bicolor allows for an unusual mix: Roses made of stainless steel and with metallic finishes in PVD enclose a coloured polyamide inlay. This creates exciting contrasts with matt surfaces that give the rose a velvety touch. The lever handle and inlay in deep black add elegant accentuation to the door. With the matt-finished nuances in brass, copper or black chrome individual design options are opened up.

Standard-compliant and versatile

The fastening technology fulfils the requirements of user category 4 according to DIN 1906 and is suitable for both the private sector and for heavily frequented office and commercial buildings.

Range 270

Range 270, designed by architect and designer Hadi Teherani, is characterised by architectural grace. The design language shows attitude through its deliberately chosen purist design. Clear edges and geometric lines seem reminiscent of his architecture. The lever handle range 270 is available with the bicolour technology as well as with the innovative mini mounting concept.

Bicolour rose

For bicolor, HEWI offers a special design solution for fixing the door handles. The extremely flat roses have an installation height of only 4 mm and are optionally available in satin stainless steel or with PVD coating.

The pre-assembled modules are connected by snap-in assembly. This ensures simple, tool-free and precise assembly, whilst removal is just as easy and quick. The bicolour rose does not require any special processing of the door leaf. The standard drill holes of the door are used for mounting.